TECHNICAL SPECIFICATION OF HERBICIDES (APPLY AS PERMANUFACTURER’S SPECIFICATION)
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ITEM
NO.

ACTIVE INGREDIENT

CONCENTRATION

21

Dicamba (Benzoic Acid) 120 G/L (As
Dimethyl Amine Salt)

2.4-D (Phenoxy Compound) 180 G/L
(As Dimethyl Amine Salt)

MCPA (Phenoxy Compound) 157.5
G/L (As Dimethyl Amine Salt)

(As Per Manufacturers
Recommendation)

Ha

22

Spraying Of Weeds Per 100m2

Using of glyphosate which does not
contain tallowamine.

As Per Manufacturers
Specification m2

23

Spraying Of Weeds per hectare with
a Glyphosate and Clethodim must
not  contain  Tallowamine
surfactants.

(Cyclohexanedione) 120 G/L
(As Per Manufacturers
Recommendation)

As Per Manufacturers
Specification Ha





